|  |  |
| --- | --- |
| **Date** |  |
| **Account Name** |  |
| **Order Reference** |  |
| **Delivery Address***(if different to account address)* |  |

****

**CRS Easylock Roman Blind Order Form**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Blind Reference** | **Blind Width** | **Blind or Chain Drop** (Please Specify which) | **Installation Height** | **Gearing (1:1 Breakaway)****(1:4 Breakaway) or**  **(1:4 NON Breakaway)** | **RH or LH Operation** | **Colour of Chain** | **Fixing screws required**No extra charge |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |

**Gearing:**

1:1 Breakaway Gearing Copes with 5KG and is supplied with an integrated breakaway within the control unit, length of operating chain shall be at least 60cm from floor.

1:4 Breakaway Gearing Copes with 7.5KG and is supplied with an integrated breakaway within the control unit, length of operating chain shall be at least 60cm from floor.

 1:4 NON Breakaway Gearing Copes with 7.5KG and is supplied with a wall retainer, length of operating chain shall be at least 150cm from floor.

**Chain Colours:**

Chrome, Brass, Antique Brass, White plastic