|  |  |
| --- | --- |
| **Date** |  |
| **Account Name** |  |
| **Order Reference** |  |
| **Delivery Address***(if different to account address)* |  |

****

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Blind Reference** | **Headrail Width** | **Required Chain Drop***See notes below in red* | **Installation Height***See notes below in red* | **1:1 Breakaway****or****1:4 Breakaway****or****1:4 non-Breakaway** *Please specify which* | **RH or LH Operation** | **Chain Colour** | **Fixing screws required**No extra charge | **Rear Breakaway?** **2 per spool are supplied****76444 for Eyelet rings****or****76666 for Roman Blind Tape****or****Or Not Required** |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |

**Roman Blind Order Form**

**Gearing:**

1:1 Breakaway Gearing Copes with 3.5KG and is supplied with an integrated breakaway within the control unit, length of operating chain shall be at least 60cm from floor.

1:4 Breakaway Gearing Copes with 10KG and is supplied with an integrated breakaway within the control unit, length of operating chain shall be at least 60cm from floor.

 1:4 NON-Breakaway Gearing Copes with 7.5KG and is supplied with a wall retainer, length of operating chain shall be at least 150cm from floor.

Install height required in order to qualify chain height is made within child safety legislation limit.

**Chain Colours:** *Chrome as standard.*

Chrome, Brass, Antique Brass, Matt Nickel, Copper & White plastic