{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":3,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":37,"n_cols":26,"rows_kept":37,"cut":false,"hidden":false,"merged":[[4,0,4,27],[14,0,14,2],[16,3,17,5],[16,2,17,2],[16,14,17,15],[8,25,8,27],[10,25,10,27],[16,0,17,1],[8,14,8,23],[16,25,17,28],[8,0,8,11],[12,25,12,27],[12,14,12,23],[12,0,12,11],[11,0,11,27],[10,0,10,11],[20,0,20,1],[16,18,17,19],[16,20,17,24],[18,20,18,24],[19,20,19,24],[20,20,20,24],[20,3,20,5],[17,12,17,13],[17,8,17,9],[16,8,16,9],[16,10,16,13],[19,3,19,5],[17,10,17,11],[18,10,18,11],[16,16,16,17],[30,14,30,26],[31,14,31,26],[32,14,32,26],[34,14,34,26],[35,14,35,26],[33,14,33,26],[22,3,22,5],[18,3,18,5],[23,3,23,5],[22,20,22,24],[23,20,23,24],[19,10,19,11],[20,10,20,11],[18,12,18,13],[19,12,19,13],[20,12,20,13],[21,12,21,13],[22,12,22,13],[23,12,23,13],[23,8,23,9],[21,10,21,11],[22,10,22,11],[16,6,16,7],[24,20,24,24],[25,20,25,24],[21,20,21,24],[19,25,19,28],[20,25,20,28],[24,25,24,28],[25,25,25,28],[18,25,18,28],[21,25,21,28],[22,25,22,28],[23,25,23,28],[23,6,23,7],[34,0,34,5],[10,14,10,23],[28,14,29,26],[22,0,22,1],[25,0,25,1],[21,0,21,1],[21,3,21,5],[25,3,25,5],[18,0,18,1],[19,0,19,1],[23,10,23,11],[24,10,24,11],[25,10,25,11],[24,12,24,13],[25,12,25,13]]}
[]
[]
[]
[]
["2740 Wave Panel Glide Measure Sheet"]
[]
[]
[]
["Date of Order: "]
[]
["Company Name: "]
["Delivery Address: "]
["Site Contact: "]
[]
["Page Number:        "]
[]
["Quantity",null," Width","Drop",null,null,"Stack       Side",null,"Inside or Outside Recess",null,"Carrier",null,null,null,null,null,"Panel Configuration",null,"Fabric Type ",null,"Fabric Colour",null,null,null,null,"Location"]
[null,null,null,null,null,null,"LH","RH","Input I or O",null,"Type A",null,"Type B",null,null,null,"Connected","Un-connected"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Notes:   ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"        Carrier A - Standard",null,null,null,null,null,"Carrier B - Optional"]
["1. This system is Top Fix hand drawn only "]
["2. Panels are fixed width at 462 mm wide"]
["3. Single stack only"]
["4. Refer to catalogue for the number of panels per system"]
["5. Track is 6010 white only"]
["6. Max. Drop 2.80 m "]
["7. Max. Width 6.0 m for connected panels"]
["8. If inside recess stated Silent Gliss will make deductions to fit within your recess"]
["9. If Outside recess stated Silent Gliss will make as finished blind width and top of headrail to bottom of the fabric panel"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}