{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":16,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":48,"n_cols":21,"rows_kept":48,"cut":false,"hidden":false,"merged":[[27,1,27,2],[28,1,28,2],[29,1,29,2],[21,1,21,2],[22,1,22,2],[23,1,23,2],[24,1,24,2],[25,1,25,2],[26,1,26,2],[5,1,5,20],[19,5,19,6],[12,1,12,14],[10,1,10,7],[16,1,16,4],[8,1,8,7],[8,10,8,12],[10,10,10,12],[14,10,14,12],[10,15,10,20],[7,15,8,20],[19,1,20,2],[14,1,14,7],[29,3,29,4],[28,7,28,8],[21,3,21,4],[23,7,23,8],[21,7,21,8],[22,3,22,4],[23,3,23,4],[22,7,22,8],[46,12,46,20],[39,12,39,20],[40,12,40,20],[43,12,43,20],[41,12,41,20],[42,12,42,20],[36,3,36,5],[32,1,32,2],[33,1,33,2],[36,9,36,20],[31,9,31,20],[32,9,32,20],[33,9,33,20],[32,3,32,5],[33,3,33,5],[34,3,34,5],[34,1,34,2],[35,3,35,5],[47,1,47,20],[19,14,19,15],[19,7,20,8],[19,9,20,9],[19,10,20,10],[19,11,20,11],[19,3,20,4],[34,9,34,20],[35,9,35,20],[31,1,31,2],[28,3,28,4],[29,7,29,8],[42,1,42,10],[35,1,35,2],[36,1,36,2],[31,3,31,5]]}
[]
[]
[]
[]
[]
[null,"Electric 4870 Roller Blind Measure Sheet"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Date Required: "]
[null,"Date of order:                  ",null,null,null,null,null,null,null,null,"Order Reference:                                             "]
[]
[null,"Company Name:                                                               ",null,null,null,null,null,null,null,null,"Contact:                                                                    ",null,null,null,null,"Telephone Number:                                                                                  "]
[]
[null,"Delivery Address:                                                                                                                                                                                                                                                                                                                                            "]
[]
[null,"Site Contact:                                                                                                                                              ",null,null,null,null,null,null,null,null,"Telephone Number:                                                                                   ",null,null,null,null,"Customer Signature:                                                                               "]
[]
[null,"Page Number:         of              "]
[]
[]
[null,"Quantity",null,"Width ",null,"Double System ",null,"Drop",null,"Fabric Name","Colour Ref","Blind Reference / Location","Inside or Outside Recess","Motor Side         Right or Left"," 4903 Bottom Bar Standard              (White or Silver)                               Optional Fabric Pocket",null,"***Motor Type     S -Standard      A-9940 Integrated ","   Standard or Reverse Rolled","Side Guided","Top or face Fixing","Fascia  "]
[null,null,null,null,null,"Left Side Width","Right Side Width",null,null,null,null,null,"Input           IR or OR","Input         R or L","Input          W or S","Input       FP              ","Input                       S or A","Input       S or R          ","Input     Y or N","Input         T or F","Input          Y or N"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"9940/0450",null,"Controls Required / 0997 Limit Setting Lead",null,null,"Qty",null,null,"Additional Information - Please ensure all text is visible "]
[]
[]
[]
[]
[]
[]
[null,"Please Note:- "]
[null,"If I entered for Inside Recess manufacturing allowances will be made and no bracket covers supplied. "]
[null,"If O entered for Outside recess size will be finished / exact size, bracket covers will be supplied additional to size."]
[null,"**If double system please state width 1 left hand section and width 2 right hand section"]
[null,"*** For operation via 0450 an 0919 receiver will be required per blind\n"]
[null,"Please consult the application chart in our Price List exc. VAT to ensure that the fabric desired can be supplied in dimensions required "]
[null,"0997 Setting lead - Please refer to current price list for pricing."]
[null,"For extra optional accessories please refer to the catalogue page"]
[null,"All dimensions to be in mm"]
[null,"For more detailed information on this system please visit our website www.silentgliss.co.uk"]