{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["4955"],"not_rendered":{"charts":0,"images":6,"macros":0,"external_links":0,"defined_names":2,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"4955","index":0,"n_rows":54,"n_cols":15,"rows_kept":54,"cut":false,"hidden":false,"merged":[[50,11,50,14],[13,12,13,14],[9,12,9,14],[13,8,13,9],[9,8,9,9],[17,13,17,14],[25,4,25,5],[53,0,53,14],[35,11,35,14],[36,11,36,14],[37,11,37,14],[38,11,38,14],[39,11,39,14],[40,11,40,14],[41,11,41,14],[43,11,43,14],[44,11,44,14],[45,11,45,14],[46,11,46,14],[47,11,47,14],[48,11,48,14],[49,11,49,14],[21,0,21,1],[21,2,21,3],[21,4,21,5],[34,2,34,3],[34,12,34,16],[22,0,22,1],[22,2,22,3],[22,4,22,5],[23,0,23,1],[23,2,23,3],[23,4,23,5],[24,0,24,1],[24,2,24,3],[24,4,24,5],[25,0,25,1],[25,2,25,3],[20,0,20,1],[20,2,20,3],[20,4,20,5],[17,0,18,1],[17,2,18,3],[17,4,18,5],[19,0,19,1],[19,2,19,3],[19,4,19,5],[17,7,18,7],[17,8,18,8],[4,0,4,16],[7,0,7,6],[9,0,9,6],[6,12,7,14],[11,0,11,14],[7,8,7,9],[13,0,13,6],[15,0,15,3],[17,6,18,6]]}
[]
[]
[]
[]
["4955 Battery Roller Blind Measure Sheet"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Date Required: "]
["Date of order:                                                        ",null,null,null,null,null,null,null,"Order Reference:"]
[]
["Company Name:                                                                                                                          ",null,null,null,null,null,null,null,"Contact:                                                                    ",null,null,null,"Telephone Number:                                                                                                    "]
[]
["Delivery Address:                                                                                                                                                                                                                                                                                                                                                                 "]
[]
["Site Contact:                                                                                                                                              ",null,null,null,null,null,null,null,"Telephone Number:                                                                                                       ",null,null,null,"Customer Signature:                                                                                       "]
[]
["Page Number:         of              "]
[]
["Quantity",null,"Width ",null,"Drop",null,"Fabric Name","Colour Ref","Blind Reference / Location","Inside                   or                                       Outside Recess","Fascia facing Front or Back","Top or Face Fix","   Standard or                 Reverse Rolled"," 4221 Bottom Bar Standard                          (White or Silver)                               Optional Fabric Pocket"]
[null,null,null,null,null,null,null,null,null,"Input                            IR or OR","Input               F or B","Input                     T or F","Input                            S or R          ","Input               W or S","Input             FP              "]
[]
[]
[]
[]
[]
[]
[]
[]
["Please Note:- "]
["* Battery always located on right hand side of blind"]
["** 3044 clamps and 11086 spacers will be provided as standard, enabling the installer to decide the most suitable method of fixing on site."]
["*** Please note that for direct fixing, the headrail profiles will NOT be pre-drilled. Installer must remove the fabric barrel and drill screw holes in the appropriate positions."]
["Please refer to the 4955 calculation chart on our website to ensure blind size and fabric combination are within the parameters of the system."]
["Please consult the application chart in our Price List exc. VAT to ensure that the fabric desired can be supplied in dimensions required "]
[]
["Max Drop"]
[null,null,null,null,null,null,null,null,null,null,null,"Additional Information"]
[]
[null,null,null,null,null,null,null,null,null,"                  "]
[]
["Please refer to the Silent Gliss fabric cards to obtain fabric thicknesses."]
[]
["System Orientation"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[" Fascia to the front with std roll",null,null,null,null,null,"  Fascia to the back with std roll","     Fascia to the front with reverse roll       Fascia to the back with reverse roll"]
[]
["For more detailed information on this system please visit our website www.silentgliss.co.uk"]