{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":37,"n_cols":24,"rows_kept":37,"cut":false,"hidden":false,"merged":[[28,3,28,5],[11,20,11,23],[9,20,9,23],[7,20,7,23],[7,10,7,16],[9,10,9,16],[11,10,11,16],[19,3,19,5],[15,17,15,18],[15,8,15,9],[16,8,16,9],[15,3,16,5],[21,8,21,9],[22,8,22,9],[23,8,23,9],[18,8,18,9],[34,15,34,22],[35,15,35,22],[36,15,36,22],[21,3,21,5],[26,3,26,5],[27,3,27,5],[27,8,27,9],[28,8,28,9],[31,15,31,22],[32,15,32,22],[33,15,33,22],[24,8,24,9],[25,8,25,9],[26,8,26,9],[24,3,24,5],[25,3,25,5],[15,2,16,2],[15,6,15,7],[17,3,17,5],[4,0,4,24],[13,0,13,2],[15,20,15,22],[7,0,7,5],[9,0,9,5],[15,23,16,23],[10,0,10,23],[11,0,11,5],[15,0,16,0],[15,10,15,12],[15,13,16,14],[17,8,17,9],[15,15,15,16],[18,3,18,5],[19,8,19,9],[20,8,20,9],[23,3,23,5],[20,3,20,5],[22,3,22,5]]}
[]
[]
[]
[]
["5300/5800 Electric Curtain Track Measure Sheet"]
[]
[]
["Date of Order:                                             ",null,null,null,null,null,null,null,null,null,"Order Reference:                                                                 ",null,null,null,null,null,null,null,null,null,"Date Required:"]
[]
["Company Name:",null,null,null,null,null,null,null,null,null,"Contact:",null,null,null,null,null,null,null,null,null,"Telephone Number:"]
["Delivery Address:"]
["Site Contact: ",null,null,null,null,null,null,null,null,null,"Telephone Number: ",null,null,null,null,null,null,null,null,null,"Customer Signature: "]
[]
["Page Number:          of    "]
[]
["System Number","*Track Colour","Quantity","Width",null,null,"Motor side ",null,"*Motor Position ",null,"Stacking Position",null,null,"Track to be Bent or Straight",null,"Fixing",null,"**5800 Only Motor Fixing",null,"**Parallel Track","Motor Type Receiver                       (External Receiver Only)",null,null,"Location"]
[null,"White (W)             or               Silver (S)",null,null,null,null,"LH","RH","Above or Below",null,"LH","RH","Pair",null,null,"Top  Clamp","*Face ","Floor","Wall","Single Track (S) or                 Parallel Track (P)","None",9940,"0450"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Notes: "]
["All curtains must be underslung",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Additional Information - Please ensure all text is visible"]
["Remember to order & list receivers /  handsets / transmitters if radio controlled option required"]
["Bent tracks MUST include template or Plot"]
["*5300 Only"]
["**5800 Only"]
["Warning - Minimum distance from track to motor of 2m for 5800 only,"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}