{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":54,"n_cols":20,"rows_kept":54,"cut":false,"hidden":false,"merged":[[36,7,36,18],[22,4,23,4],[23,11,24,11],[22,6,24,6],[22,10,24,10],[22,7,22,8],[23,7,24,8],[25,7,25,8],[26,7,26,8],[27,7,27,8],[28,7,28,8],[29,7,29,8],[30,7,30,8],[31,7,31,8],[32,7,32,8],[8,0,8,20],[24,13,24,14],[22,9,24,9],[22,19,24,20],[23,13,23,14],[23,15,24,15],[23,12,24,12],[23,17,24,17],[23,16,24,16],[22,5,24,5],[22,18,24,18],[22,2,24,2],[22,1,24,1],[53,0,53,7],[49,0,49,7],[50,0,50,2],[51,0,51,2],[51,3,51,7],[52,3,52,7],[50,3,50,7],[52,0,52,2],[38,7,38,18],[40,0,41,6],[41,7,41,18],[39,7,39,18],[40,7,40,18],[22,0,24,0],[22,3,24,3],[22,12,22,15],[53,9,53,12],[53,13,53,18],[49,9,49,18],[50,9,50,12],[51,9,51,12],[52,9,52,12],[50,13,50,18],[51,13,51,18],[52,13,52,18],[42,7,42,18],[43,7,43,18],[44,7,44,18],[37,7,37,18],[34,7,34,8],[11,15,12,16],[11,17,12,20],[14,15,14,16],[13,17,14,20],[18,15,18,16],[17,17,18,20],[17,9,18,13],[13,8,14,13],[11,9,12,13],[12,7,12,8],[18,7,18,8],[34,19,34,20],[33,19,33,20],[29,19,29,20],[28,19,28,20],[11,1,12,5],[13,1,14,5],[15,1,16,20],[17,1,18,5],[33,7,33,8],[27,19,27,20],[32,19,32,20],[31,19,31,20],[30,19,30,20],[26,19,26,20],[25,19,25,20]]}
[]
[]
[]
[]
[]
[]
[]
[]
["Metropole Measure Sheet - System 6120"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Date Required:"]
["Date of Order:  ",null,null,null,null,null,null,"Order Reference: "]
[]
["Company Name: ",null,null,null,null,null,null,"Contact:",null,null,null,null,null,null,null,"Telephone Number:"]
[]
["Delivery Address:    "]
[]
["Site Contact: ",null,null,null,null,null,null,"Telephone Number: ",null,null,null,null,null,null,null,"Customer Signature:"]
[]
[]
[]
["Colour","Qty","Overall Length","**Installation Height                               Child Safety Legislation -         EN 13120","Finial","Size Given is Including (Inc)                      or                             Excluding (Exc) Finials","Cord Colour                      B or W","Input                                         T or F",null,"Bracket number if known or projection                                            in mm","Cord Drop","Pole Supplied","Glider Type",null,null,null,"Method","Input                        LH / RH or B","Child Safety Device (Integral 10483)   (Available with Colorama Silent Gliss curtains only)","Location"]
[null,null,null,null,null,null,null,"****Top (6138P) \nor \nFace (11206) Standard Fixing brackets",null,null,null,"***Bent or Straight","Standard 6143","*****Wave",null,"Other Please specify","LH / RH / Pair                     or                                      Centre Stacking","* Left / right or both side operation"]
[null,null,null,null,"A1 Flush                     A2 Stud                   other please specify",null,null,null,null,null,null,null,null,"                                                    60mm             80mm"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Please Note:",null,null,null,null,null,null,"Any additional Notes - Please ensure all text is visible "]
["For multiple stack please include diagram"]
["* If B for both, intermediate pulley will be added at extra cost"]
["** If Installation Height is known, cord drops will comply with EN13120 "]
["*** If bent poles required, 0537 brackets will be supplied as standard.  Please confirm if a plot or template will be supplied."]
[]
["**** If finials required 0335 top fix brackets will be supplied"]
["***** If Face fix 3135 bracket = 60mm"]
["       If Face fix 3136 bracket = 80mm"]
[]
[]
["Child Safety Legislation - EN 13120"]
[]
["Operating loop for Child Safety Device",null,null,null,null,null,null,null,null,"Operating loop for cord retainer"]
["Installation height",null,null,"Chain Length",null,null,null,null,null,"Installation Height",null,null,null,"Cord length"]
["Known",null,null,"Distance from floor to bottom of pull cords shall be at least 0.6m",null,null,null,null,null,"Known",null,null,null,"Distance from floor to bottom of operating chain shall be at least 1.5m"]
["Unknown",null,null,"Less than or equal to 2/3rd drop of the blind",null,null,null,null,null,"Not Known drop ≤ 2.5m",null,null,null,"length of operating chain loop shall be ≤ 1m"]
[null,null,null,null,null,null,null,null,null,"Not known drop > 2.5m",null,null,null,"Shall be ≤ drop of blind less 1.5m"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}