{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":16,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":45,"n_cols":25,"rows_kept":45,"cut":false,"hidden":false,"merged":[[44,1,44,24],[28,1,28,3],[26,4,26,6],[26,7,26,8],[31,4,31,7],[31,1,31,3],[29,1,29,3],[30,1,30,3],[24,1,24,3],[25,1,25,3],[21,7,21,8],[22,7,22,8],[23,7,23,8],[24,7,24,8],[36,1,36,11],[30,14,30,24],[30,4,30,7],[31,14,31,24],[25,7,25,8],[42,15,42,24],[34,15,34,24],[35,15,35,24],[39,15,39,24],[36,15,36,24],[37,15,37,24],[3,1,3,24],[26,9,26,10],[19,4,19,6],[21,9,21,10],[19,9,19,10],[20,4,20,6],[21,4,21,6],[20,9,20,10],[19,7,19,8],[20,7,20,8],[13,1,13,9],[20,1,20,3],[21,1,21,3],[16,7,18,8],[26,1,26,3],[19,1,19,3],[16,4,18,6],[16,1,18,3],[28,14,28,24],[29,14,29,24],[28,4,28,7],[29,4,29,7],[16,23,17,23],[16,24,17,24],[16,9,18,10],[16,20,16,22],[16,17,17,19],[16,16,17,16],[16,15,17,15],[16,14,17,14],[22,1,22,3],[23,1,23,3],[6,1,6,2],[8,1,8,3],[10,1,10,3],[12,1,12,2],[14,1,14,2],[14,3,14,4],[6,3,6,9],[8,4,8,9],[10,4,10,24],[12,3,12,9],[6,16,6,17],[8,16,8,18],[12,16,12,18],[6,18,6,24],[8,19,8,24],[12,19,12,24],[23,11,23,12],[24,11,24,12],[25,11,25,12],[26,11,26,12],[6,11,6,12],[12,11,12,12],[8,12,8,13],[16,11,18,12],[19,11,19,12],[20,11,20,12],[21,11,21,12],[22,11,22,12],[16,13,18,13],[23,17,23,18],[24,17,24,18],[25,17,25,18],[26,17,26,18],[18,17,18,18],[19,17,19,18],[20,17,20,18],[21,17,21,18],[22,17,22,18]]}
[]
[]
[]
[null,"Electric 4880 Roller Blind Measure Sheet"]
[]
[]
[null,"Date of order:                                                        ",null,null,null,null,null,null,null,null,null,"Order Reference:                                             ",null,null,null,null,"Date Required: "]
[]
[null,"Company Name:                                                                                                                        ",null,null,null,null,null,null,null,null,null,"Contact:                                                                                        ",null,null,null,null,"Telephone Number:                                                                                  "]
[]
[null,"Delivery Address:                                                                                                                                                                                                                                                                                                                                            "]
[]
[null,"Site Contact:                                                                                                                                                                                      ",null,null,null,null,null,null,null,null,null,"Telephone Number:                                                                                   ",null,null,null,null,"Customer Signature:                                                                               "]
[]
[null,"Page Number:",null,null,null,"of"]
[]
[null,"Quantity ",null,null,"Width ",null,null,"Drop",null,"Fabric Name",null,"Colour Ref",null,"Blind Reference / Location","Inside or Outside Recess","Motor Side     Right or Left","Top or face Fixing"," 4903 Bottom Bar Standard              (White or Silver)                               Optional Fabric Pocket",null,null,"Motor Options",null,null,"   Standard or Reverse Rolled","Side Guided "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"*Motor Type     S -Standard                      (Mains 240V)           Series 20","**Motor Type         Integrated 9940   Mains or 24V    Series 40     ","Smart"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Input           IR or OR","Input         R or L","Input         T or F","Input          W or S",null,"Input       FP              ","Input                       S ","Input                      Mains or 24V","Input                       Y or N","Input       S or R          ","Input           Y or N"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"9940/0450",null,null,"Controls Required ",null,null,null,"Qty",null,"Test Lead - 0997","Test Lead - TT Pro",null,null,"Additional Information - Please ensure all text is visible "]
[]
[]
[]
[]
[null,"Please Note:- "]
[null,"If I entered for Inside Recess manufacturing allowances will be made and no bracket covers supplied. "]
[null,"If O entered for Outside recess size will be finished / exact size, bracket covers will be supplied additional to size."]
[null,"* For operation via 0450 an 0919 receiver will be required per blind use with Series 20 only"]
[null,"** 9940 Integrated Series 40 motors are supplied with dry contact connectivity as standard"]
[null,"0997 Setting lead for Series 20- 240V Std Motors "]
[null,"TT Pro Setting leads required for Integrated 9940 Series 40 or Smart Motors"]
[null,"For extra optional accessories please refer to the catalogue page"]
[null,"All dimensions to be in mm"]
[null,"Please consult the application chart in our Price List exc. VAT to ensure that the fabric desired can be supplied in dimensions required "]
[]
[null,"For more detailed information on this system please visit our website www.silentgliss.co.uk"]