{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":16,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":55,"n_cols":25,"rows_kept":55,"cut":false,"hidden":false,"merged":[[4,1,4,25],[18,15,19,15],[18,8,19,8],[20,6,20,7],[21,6,21,7],[22,6,22,7],[23,6,23,7],[24,6,24,7],[18,24,19,25],[20,24,20,25],[21,24,21,25],[9,1,9,3],[11,1,11,3],[7,1,7,2],[24,3,24,5],[25,3,25,5],[26,3,26,5],[7,3,7,7],[9,4,9,7],[13,1,13,2],[15,1,15,2],[18,3,19,5],[20,3,20,5],[21,3,21,5],[22,24,22,25],[54,1,54,25],[18,18,18,19],[18,6,19,7],[18,9,19,9],[18,12,19,12],[28,6,28,7],[23,24,23,25],[24,24,24,25],[53,15,53,25],[38,15,38,25],[25,24,25,25],[52,13,52,15],[51,13,51,15],[22,3,22,5],[23,3,23,5],[25,6,25,7],[26,6,26,7],[27,3,27,5],[28,3,28,5],[26,24,26,25],[51,1,51,4],[52,1,52,4],[49,6,49,10],[50,6,50,10],[51,6,51,10],[50,13,50,15],[49,13,49,15],[27,6,27,7],[39,15,39,25],[42,15,42,25],[40,15,40,25],[41,15,41,25],[35,3,35,23],[30,3,30,23],[31,3,31,23],[32,3,32,23],[27,24,27,25],[28,24,28,25],[33,3,33,23],[49,1,49,4],[50,1,50,4],[34,3,34,23],[27,1,27,2],[28,1,28,2],[18,1,19,2],[20,1,20,2],[21,1,21,2],[22,1,22,2],[23,1,23,2],[24,1,24,2],[25,1,25,2],[26,1,26,2],[24,10,24,11],[25,10,25,11],[26,10,26,11],[27,10,27,11],[28,10,28,11],[18,10,19,11],[20,10,20,11],[21,10,21,11],[22,10,22,11],[23,10,23,11],[7,10,7,11],[13,10,13,11],[7,19,7,20],[9,19,9,21],[13,19,13,21],[7,21,7,25],[9,22,9,25],[13,22,13,25],[7,12,7,14],[9,11,9,14],[13,12,13,14],[11,4,11,25],[13,3,13,7],[28,20,28,21],[23,20,23,21],[24,20,24,21],[25,20,25,21],[26,20,26,21],[27,20,27,21],[18,20,18,21],[19,20,19,21],[20,20,20,21],[21,20,21,21],[22,20,22,21]]}
[]
[]
[]
[]
[null,"Manual 4910 Roller Blind Measure Sheet"]
[]
[]
[null,"Date of order:",null,null,null,null,null,null,null,null,"Order Reference:                                  ",null,null,null,null,null,null,null,null,"Date Required: "]
[]
[null,"Company Name: ",null,null,null,null,null,null,null,null,"Contact:                                                                   ",null,null,null,null,null,null,null,null,"Telephone Number:                                                                                  "]
[]
[null,"Delivery Address:                                                                                                                                                                                                                                                                                                                                                                                                 "]
[]
[null,"Site Contact:                                                                                                                                                                ",null,null,null,null,null,null,null,null,"Telephone Number:                                                                                   ",null,null,null,null,null,null,null,null,"Customer Signature:                                                                               "]
[]
[null,"Page Number:     ",null,null,"of"]
[]
[]
[null,"Quantity",null,"Width ",null,null,"Drop",null,"Installation Height : EN13120  -see notes below \n \n","Fabric Name","Colour Ref",null,"Blind Reference / Location","Inside or Outside Recess","Top or Face Fixing","Chain Length","Chain Side Right or Left","   Standard or Reverse Rolled"," 4221 Bottom Bar Standard              (White or Silver)                               Optional Fabric Pocket",null,"Side Guided",null,"*Facia","Continuous Headrail","\n*Child Safety\n\nSafety Device (10482)               Chain Break Connector (10486)     N/A - Child Safe Chain Length     "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Input           IR or OR","Input                    T or F",null,"Input            R or L","Input       S or R          ","Input          W or S","Input       FP              ","Input                     Y or N",null,"Input                                    Y or N","Input               Y or N"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,"Additional Information - Please ensure all text is visible "]
[]
[]
[]
[]
[]
[]
[null,"Please Note:- "]
[null,"If I entered for Inside Recess manufacturing allowances will be made and bracket covers supplied. "]
[null,"If O entered for Outside recess size will be finished / exact size, bracket covers will be supplied additional to size."]
[null,"Please consult the application chart in our Price List exc. VAT to ensure that the fabric desired can be supplied in dimensions required "]
[null,"For extra optional accessories please refer to the catalogue page"]
[null,"Chain retainers supplied as standard"]
[null,"All dimensions to be in mm"]
[null,"*Facia, if required, is (as standard) to the front of the system"]
[]
[null,"Child Safety Legislation - EN 13120"]
[]
[null,"Operating loop for Child Safety Device",null,null,null,null,null,null,null,null,null,null,null,"Operating loop for chain retainer"]
[null,"Installation height",null,null,null,null,"Chain length",null,null,null,null,null,null,"Installation height",null,null,"Chain length"]
[null,"Known",null,null,null,null,"Distance from floor to bottom of pull cords shall be at least 0.6m",null,null,null,null,null,null,"Known",null,null,"Distance from floor to bottom of operating chain shall be at least 1.5m"]
[null,"Unknown",null,null,null,null,"Less than or equal to 2/3rd drop of the blind",null,null,null,null,null,null,"Not known drop ≤ 2.5 m",null,null,"Length of operating chain loop shall be ≤ 1m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Not known Drop ˃ 2.5 m",null,null,"Shall be ≤ drop of blind less 1.5 m"]
[]
[null,"For more detailed information on this system please visit our website www.silentgliss.co.uk"]