{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["2730"],"not_rendered":{"charts":0,"images":4,"macros":0,"external_links":1,"defined_names":3,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"2730","index":0,"n_rows":57,"n_cols":7,"rows_kept":57,"cut":false,"hidden":false,"merged":[[1,6,1,11],[2,6,2,11]]}
[]
[null,"Silent Gliss 2730",null,"Rev 1 / November 09",null,"Customer:","Sample calculation (No deductions calculated)"]
[null,"Calculation Chart",null,null,null,"Fabric type:","-"]
[null,"System Parameter:"]
[null,"System width",250,"cm"]
[null,"System height",230,"cm"]
[null,"Number of panels",3,"Panels"]
[null,"Number of channels",3,"-"]
[null,"Stacking","-","-"]
[null,"Stack side","free floating","-"]
[null,"Profile colour","RAL 9010","-"]
[null,"Fitting","ceiling","-"]
[null,"System Calculation \"Free floating\":"]
[null,"Profile length",{"$f":"C5-0.8","v":249.2},"cm"]
[null,"Fabric height (incl. fabric carrier)",{"$f":"C6-3.5","v":226.5},"cm"]
[null,"Carrier length/Fabric width",{"$f":"ODD(ROUNDDOWN(((((C5-2)+((C7-1)*(11.8)))/C7))/2,0)*2)","v":91},"cm"]
[null,"Overlapping X",{"$f":"(((C16*C7)-(C5-2))/(C7-1))","v":12.5},"cm"]
[null,"System Calculation \"Connected\":"]
[null,"Profile length",{"$f":"C5-0.8","v":249.2},"cm"]
[null,"Fabric height (incl. fabric carrier)",{"$f":"C6-3.5","v":226.5},"cm"]
[null,"Carrier length/Fabric width",{"$f":"ODD(ROUNDDOWN(((((C5-2)+((C7-1)*(11.8)))/C7))/2,0)*2)","v":91},"cm"]
[null,"Overlapping X",{"$f":"((C21*C7)-(C5-2))/(C7-1)","v":12.5},"cm"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null," "]