{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":48,"n_cols":29,"rows_kept":48,"cut":false,"hidden":false,"merged":[[19,1,19,2],[20,1,20,2],[21,1,21,2],[22,1,22,2],[14,22,15,23],[16,22,16,23],[17,22,17,23],[18,22,18,23],[19,22,19,23],[20,22,20,23],[21,22,21,23],[22,22,22,23],[12,24,12,25],[14,1,15,2],[16,1,16,2],[17,1,17,2],[18,1,18,2],[8,0,8,1],[10,0,10,1],[6,12,6,13],[12,12,12,13],[5,21,6,22],[8,21,8,23],[12,21,12,23],[6,1,6,9],[8,2,8,9],[10,2,10,25],[12,1,12,9],[6,14,6,16],[8,13,8,16],[12,14,12,16],[5,23,6,25],[8,24,8,25],[14,17,14,19],[46,5,46,14],[44,5,44,14],[44,0,44,4],[45,0,45,4],[46,0,46,4],[14,13,14,14],[14,15,14,16],[16,7,16,8],[16,5,16,6],[18,5,18,6],[17,7,17,8],[18,7,18,8],[17,5,17,6],[47,19,47,28],[44,15,44,18],[45,15,45,18],[46,15,46,18],[47,15,47,18],[46,19,46,28],[44,19,44,28],[45,19,45,28],[14,10,15,10],[28,14,28,22],[45,5,45,14],[19,5,19,6],[19,7,19,8],[21,5,21,6],[34,17,35,19],[22,7,22,8],[21,7,21,8],[22,5,22,6],[24,14,24,22],[25,14,25,22],[26,14,26,22],[27,14,27,22],[20,5,20,6],[20,7,20,8],[3,0,3,28],[14,24,15,24],[14,0,15,0],[14,12,15,12],[14,25,14,28],[14,4,15,4],[14,5,15,6],[14,7,15,8],[14,9,15,9],[14,11,15,11],[14,3,15,3],[14,20,14,21]]}
[]
[]
[]
["2700 Panel Glide Measure Sheet"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Date Required: "]
["Date of Order:",null,null,null,null,null,null,null,null,null,null,null,"Order Reference: "]
[]
["Company Name:",null,null,null,null,null,null,null,null,null,null,null,"Contact: ",null,null,null,null,null,null,null,null,"Telephone Number:"]
[]
["Delivery Address: "]
[]
["Site Contact:",null,null,null,null,null,null,null,null,null,null,null,"Telephone Number: ",null,null,null,null,null,null,null,null,"Customer Signature: "]
[]
["System","Operation:\nHand / \nCord / \nElectric",null,"Qty","*Installation Height: EN 13120","Width",null,"Drop",null,"Panel Qty.","Panel Width","Over-lap","No. of channels","Recess\nplease tick",null,"Operation side\nplease tick",null,"Stacking\nplease tick",null,null,"Fixing\nplease tick",null,"Fabric",null,"Draw Rod / Cord Drop length if applicable","Motor Type / Integrated Receiver"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Inside","Outside","LH","RH","LH","RH","Pair","Top","Face",null,null,null,"Std Motor","9940\n(A)","0450\n(B)","Smart"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Additional Information - please ensure all text is visible "]
[]
["Notes: "]
["If draw rod required please specify, type, length and quantity"]
["White profile is supplied as standard"]
["If I entered for Inside Recess manufacturing allowances will be made.  Drop given must be top of Headrail to floor."]
["If O entered for Outside recess size will be finished / exact size, drop given must be top of headrail to bottom of fabric"]
["If electrically operated please add 5600 track to cost (5600 with radio module, if radio controlled).  Wiring diagrams can be sent on request from Customer Services"]
["On hand operated system please state if panels are connected (Standard) or unconnected"]
["Remember to order and list handsets / transmitters separately if radio controlled option required"]
["System Options: 2700HD, 2700CD, 2700EL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"For 2700EL Motor Types:",null,null,"Standard 9060 motor for standard switch operation"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"For radio control option 9063EL, please select (A) for 9940"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"For radio control option 9063, please select (B) for 0450"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"For Smart control option select Smart"]
[null,null,null,"* If Installation Height is known, cord drops will comply to EN13120 "]
[null,null,null,null,null,"This measure sheet MUST be accompanied by a completed 2700 calculation sheet, this can be found on our website or from our Broadstairs office"]
[]
["Child Safety Legislation - EN 13120"]
[]
["Operating loop for Child Safety Device",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Operating loop for cord retainer"]
["Installation height",null,null,null,null,"Chain length",null,null,null,null,null,null,null,null,null,"Installation height",null,null,null,"Cord length"]
["Known",null,null,null,null,"Distance from floor to bottom of pull cords shall be at least 0.6m",null,null,null,null,null,null,null,null,null,"Known",null,null,null,"Distance from floor to bottom of operating chain shall be at least 1.5 m"]
["Unknown",null,null,null,null,"Less than or equal to 2/3rd drop of the blind",null,null,null,null,null,null,null,null,null,"Not known drop ≤ 2.5 m",null,null,null,"Length of operating chain loop shall be ≤ 1m"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Not known Drop ˃ 2.5 m",null,null,null,"Shall be ≤ drop of blind less 1.5 m"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}