{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":38,"n_cols":20,"rows_kept":38,"cut":false,"hidden":false,"merged":[[27,17,27,18],[27,19,27,20],[7,8,7,10],[13,8,13,10],[28,8,28,9],[27,8,27,9],[26,8,26,9],[17,13,18,14],[19,13,19,14],[20,13,20,14],[21,13,21,14],[22,13,22,14],[23,13,23,14],[24,13,24,14],[25,13,25,14],[26,13,26,14],[27,13,27,14],[28,13,28,14],[23,8,23,9],[24,8,24,9],[25,8,25,9],[26,6,26,7],[27,6,27,7],[28,0,28,1],[17,6,19,7],[20,6,20,7],[21,6,21,7],[22,6,22,7],[23,6,23,7],[24,6,24,7],[25,6,25,7],[28,6,28,7],[23,0,23,1],[24,0,24,1],[25,0,25,1],[26,0,26,1],[27,0,27,1],[13,15,13,20],[17,0,19,1],[20,0,20,1],[21,0,21,1],[22,0,22,1],[17,8,19,9],[20,8,20,9],[21,8,21,9],[22,8,22,9],[9,0,9,1],[11,0,11,1],[7,6,7,7],[13,6,13,7],[6,13,7,13],[9,13,9,14],[13,13,13,14],[7,1,7,4],[9,2,9,4],[11,2,11,20],[13,1,13,4],[9,7,9,10],[7,14,7,20],[9,15,9,20],[40,3,40,5],[41,3,41,5],[4,0,4,20],[14,0,14,3],[14,19,14,21],[17,2,19,2],[17,3,19,3],[17,4,19,4],[47,0,47,2],[44,3,44,6],[45,3,45,6],[46,3,46,6],[47,3,47,6],[44,0,44,2],[45,0,45,2],[46,0,46,2],[43,0,43,11],[41,0,41,2],[40,0,40,2],[39,3,39,5],[17,5,19,5],[20,19,20,20],[21,19,21,20],[17,10,18,10],[17,11,18,11],[17,12,18,12],[20,17,20,18],[21,17,21,18],[17,19,18,20],[19,19,19,20],[23,17,23,18],[24,17,24,18],[18,17,18,18],[17,15,17,18],[19,17,19,18],[42,13,42,19],[36,9,37,9],[38,10,38,11],[40,10,40,11],[41,10,41,11],[42,10,42,11],[39,10,39,11],[36,10,37,11],[36,13,37,19],[38,13,38,19],[39,13,39,19],[40,13,40,19],[41,13,41,19],[36,12,37,12],[34,10,34,11],[30,9,31,9],[30,10,31,11],[30,12,31,12],[22,19,22,20],[23,19,23,20],[32,10,32,11],[25,17,25,18],[25,19,25,20],[24,19,24,20],[26,19,26,20],[28,19,28,20],[26,17,26,18],[28,17,28,18],[33,10,33,11],[22,17,22,18]]}
[]
[]
[]
[]
["Motorised Roman Blind Measure Sheet"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Date Required:"]
["Date of Order:                                             ",null,null,null,null,null,"Order Reference:                                                                 "]
[]
["Company Name:",null,null,null,null,null,"Contact:",null,null,null,null,null,null,"Telephone Number:"]
[]
["Delivery Address:"]
[]
["Site Contact: ",null,null,null,null,null,"Telephone Number: ",null,null,null,null,null,null,"Customer Signature:"]
["Page Number:          of    ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Customer Signature: "]
[]
[]
["System Type\n2350 Motorised\n2345 - Battery",null,"H = Hard fold\nS = Soft Fold\n*SH = Semi Hard fold","Qty","Width","Drop","Fabric",null,"Location",null,"Inside or Outside recess","2350 Only LH or RH Operation","Top or Face Fixing","Lining Input  ",null,"Motor Options 2350 only",null,null,null,"Side Guided"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"**Motor Type\nS - Standard\nMains 240V","*** Motor Type\nIntegrated 9940\nMains or 24V                    ","Smart"]
[null,null,null,null,null,null,null,null,null,null,"Input\nI or O","Input\nLH or RH","Input\nT or F","UN = Unlined\nCR = Cream\nW   = White\nBC = B/out Cream\nBW = B/out white\nBL = Black",null,"Input\nS","Input\nMains or 24V","Input\nY or N",null,"Input\nY / N"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Please Note:","Blackout lining is available at extra cost",null,null,null,null,null,null,null,"9940/0450","Controls Req.d",null,"Qty"]
[null,"If Inside recess manufacturing allowances will be made"]
[null,"If Outside recess blind is made to finished size"]
[null,"* Semi hard fold is Silent Gliss standard    **costs may apply"]
[]
[null,"For Operation via 0450 an 0919 recaiver will be required per blind"]
[null,"*** 9940 Series 40 integrated motors are supplied with dry contact connectivity as standard",null,null,null,null,null,null,null,"Test lead - 0997","Test lead - TTPro",null,"Qty","Additional Information - Please ensure all text is visible"]
[null,"0997 setting lead for Standard 20 series motors - TT PRO are required for Series 40 and Smart Motors "]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}