{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":47,"n_cols":22,"rows_kept":47,"cut":false,"hidden":false,"merged":[[22,17,22,18],[23,17,23,18],[24,17,24,18],[25,17,25,18],[22,0,22,1],[23,0,23,1],[24,0,24,1],[25,0,25,1],[18,10,19,11],[20,10,20,11],[21,10,21,11],[22,10,22,11],[23,10,23,11],[24,10,24,11],[25,10,25,11],[15,16,15,17],[15,18,15,21],[18,0,19,1],[20,0,20,1],[21,0,21,1],[18,17,18,18],[19,17,19,18],[20,17,20,18],[21,17,21,18],[15,1,15,7],[9,10,9,11],[9,12,9,14],[11,11,11,14],[15,10,15,11],[15,12,15,14],[11,0,11,1],[13,0,13,1],[9,1,9,7],[11,2,11,7],[13,2,13,21],[8,16,9,16],[8,17,9,21],[11,16,11,17],[11,18,11,21],[36,14,36,21],[32,14,32,21],[34,14,34,21],[46,0,46,10],[35,0,35,10],[38,0,38,12],[42,0,42,10],[43,0,43,5],[44,0,44,5],[45,0,45,5],[33,0,33,12],[34,0,34,12],[35,14,35,21],[46,15,46,21],[43,15,43,21],[37,2,37,21],[18,21,19,21],[18,2,19,2],[20,4,20,5],[20,6,20,7],[18,4,19,5],[18,6,19,7],[18,9,19,9],[21,6,21,7],[22,4,22,5],[23,4,23,5],[24,4,24,5],[23,6,23,7],[4,2,4,21],[43,6,43,10],[44,15,44,21],[18,12,19,12],[43,12,43,14],[44,6,44,10],[42,12,42,21],[18,13,19,13],[25,4,25,5],[18,8,19,8],[18,14,19,14],[45,6,45,10],[45,15,45,21],[31,14,31,21],[33,14,33,21],[28,2,28,21],[29,14,29,21],[30,14,30,21],[21,4,21,5],[22,6,22,7],[25,6,25,7],[24,6,24,7]]}
[]
[]
[]
[]
[null,null,"Venetian Blind Measure Sheet"]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Date Required:"]
["Date of Order:",null,null,null,null,null,null,null,null,null,"Order Reference:"]
[]
["Company Name:",null,null,null,null,null,null,null,null,null,"Contact:",null,null,null,null,null,"Telephone Number:"]
[]
["Delivery Address:"]
[]
["Site Contact:",null,null,null,null,null,null,null,null,null,"Telephone Number: ",null,null,null,null,null,"Customer Signature: "]
[]
[]
["Product Reference:                                   8110pc / 8250 / 8300 / 8910 / 8960",null,"Qty","*Child Safety Device (Integral 10482)","Width",null,"Drop",null,"Slat Colour or Timber Reference","Slat Type:                                                WD Wood or                               AL aluminium or                                                         Tape (50mm only)","If Taped state colour of tape",null,"Slat Size    16, 25 or 50mm","Installation Height : EN13120 - see notes below","Location / any other comments","Inside or Outside recess","LH / RH Operation Side / Motor side","Motor Options            ",null,"Cable Exit","Wand / Cord / Chain Drop if non std","Side Guided                         Y or N"]
[null,null,null,"Y / N",null,null,null,null,null,null,null,null,null,null,null,"Input                                     I or O     ","Input                                       LH or RH","S = Std                            A = 9940",null,"A = Left Back          B = Right Back                           C = Left Top                                 D = Right Top","Drop"]
[]
[]
[]
[]
[]
[]
[]
["Please Note:- ",null,"If I entered for Inside Recess, manufacturing allowances will be made."]
[null,null,"If O entered for Outside recess, size will be finished / exact size."]
[null,null,"* Child Safety Device applicable to System 8300 only",null,null,null,null,null,null,null,null,null,null,null,"Additional Information - Please ensure all text is visible"]
[null,null," 8110pc only available for commercial sites with a valid Risk Assesment"]
[null,null,"Remember to order & list handsets / transmitters if radio controlled option required."]
[]
["If 8110PC, please specify wand drop. Note: due to nature of system wand will always be 130mm longer than that stated below."]
["Option size 0 = 225mm, 1 = 385mm,  2 = 585mm, 3 = 785mm, 4 = 985mm, 5 = 1185mm, 6 = 1385mm, 7 = 1585mm, 8 = 1800mm"]
["All wands would normally be operated at around chest height."]
["If 8910 or 8960 - 50 mm slats only"]
[]
["Side guided or perforated are available at extra cost on certain blinds, please consult your price list or contact Silent Gliss Sales."]
[]
["Child Safety Legislation - EN 13120"]
[]
["Operating loop for Child Safety Device",null,null,null,null,null,null,null,null,null,null,null,"Operating loop for chain retainer"]
["Installation height",null,null,null,null,null,"Chain length",null,null,null,null,null,"Installation height",null,null,"Chain length"]
["Known",null,null,null,null,null,"Distance from floor to bottom of pull cords shall be at least 0.6m",null,null,null,null,null,"Known",null,null,"Distance from floor to bottom of operating chain shall be at least 1.5 m"]
["Unknown",null,null,null,null,null,"Less than or equal to 2/3rd drop of the blind",null,null,null,null,null,"Not known drop ≤ 2.5 m",null,null,"Length of operating chain loop shall be ≤ 1m"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Not known Drop ˃ 2.5 m",null,null,"Shall be ≤ drop of blind less 1.5 m"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}