{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":2,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":57,"n_cols":20,"rows_kept":57,"cut":false,"hidden":false,"merged":[[35,1,35,3],[36,1,36,3],[37,1,37,3],[38,1,38,3],[39,1,39,3],[29,13,29,14],[30,13,30,14],[31,13,31,14],[32,13,32,14],[33,13,33,14],[23,13,24,14],[25,13,25,14],[26,13,26,14],[27,13,27,14],[28,13,28,14],[32,0,32,1],[33,0,33,1],[23,7,24,8],[25,7,25,8],[26,7,26,8],[27,7,27,8],[28,7,28,8],[29,7,29,8],[30,7,30,8],[31,7,31,8],[32,7,32,8],[33,7,33,8],[27,0,27,1],[28,0,28,1],[29,0,29,1],[30,0,30,1],[31,0,31,1],[8,14,9,17],[11,12,11,14],[11,15,11,17],[15,12,15,14],[15,15,15,17],[9,9,9,10],[11,7,11,10],[15,6,15,8],[15,9,15,10],[8,12,9,13],[56,11,56,18],[55,11,55,18],[56,0,56,8],[54,3,54,8],[53,3,53,8],[55,3,55,8],[23,3,24,3],[23,4,24,4],[23,6,24,6],[53,0,53,2],[54,0,54,2],[55,0,55,2],[54,11,54,18],[9,19,15,21],[53,9,53,10],[53,11,53,18],[45,13,45,21],[46,13,46,21],[47,13,47,21],[49,13,49,21],[23,11,24,11],[23,9,24,9],[23,15,23,17],[44,13,44,21],[13,2,13,17],[23,2,24,2],[43,13,43,21],[35,8,35,16],[36,8,36,16],[37,8,37,16],[38,8,38,16],[39,8,39,16],[23,0,24,1],[25,0,25,1],[26,0,26,1],[11,0,11,1],[13,0,13,1],[9,1,9,4],[11,2,11,4],[15,1,15,4],[9,6,9,7]]}
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,"Vertical Blind Measure Sheet"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Date Required: "]
["Date of Order: ",null,null,null,null,null,"Order Reference:",null,null,null,null,null,null,null,null,null,null,null,null,"Operating Methods:  All views from room side.  Where more than one stack is involved the operating methods below assume equal numbers of louvres in each stack.  Unequal draw is also possible.  Please consult your supplier."]
[]
["Company Name:",null,null,null,null,null,"Contact:",null,null,null,null,null,"Telephone Number:"]
[]
["Delivery Address:"]
[]
["Site Contact:",null,null,null,null,null,"Telephone Number:",null,null,null,null,null,"Customer Signature: "]
[]
[]
[]
[]
[]
[]
[]
["Product Reference \n2810, 2900, 2950",null,"Qty","Installation Height: EN13120\nsee below","Headrail Colour","Louvre size","Width","Drop",null,"Fabric Colour Ref.","Inside or Outside recess","Location","Stack Method\nsee right","Chain or Crank drop",null,"Motor/Receiver Type \n(Please Tick)",null,null,"Top or *Face fixing"]
[null,null,null,null,null,"Input 89 / 127mm",null,null,null,null,"Input\nI or O",null,"Input\n01 - 10",null,null,"Std 9090",9940,"0450","Input\nT or F"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["9940/0450","Controls Required / 0997 Limit     Setting Lead",null,null,"Qty",null,null,null,"Additional Information - Please ensure all text is visible"]
[]
[]
[]
[]
[]
[]
["Notes: "]
["If Inside recess stated Silent Gliss will make deductions to fit within your recess"]
["If Outside recess stated Silent Gliss will make as finished blind width and top of headrail to bottom of louvre"]
["If bent 2900 / 2950 system is required for bay window or gradual curve please supply an accurate drawing or template. 2810 systems cannot be bent."]
["*Additional cost for face fixing brackets"]
[]
[]
[]
["Child Safety Legislation - EN 13120"]
[]
["Operating loop for Child Safety Device",null,null,null,null,null,null,null,null,"Operating loop for chain retainer"]
["Installation height",null,null,"Chain Length",null,null,null,null,null,"Installation height",null,"Chain length"]
["Known",null,null,"Distance form floor to bottom of pull cords shall be at least 0.6m",null,null,null,null,null,"Known",null,"Distance from floor to bottom of operating chain shall be at least 1.5 m"]
["Unknown",null,null,"Less than or equal to 2/3rd drop of the blind",null,null,null,null,null,"Not known drop ≤ 2.5 m",null,"Length of operating chain loop shall be ≤ 1m"]
[null,null,null,null,null,null,null,null,null,"Not known Drop ˃ 2.5 m",null,"Shall be ≤ drop of blind less 1.5 m"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}